{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M3V1B9","2MXM50M2V1B9"]
["Dimensioni","Unità","","Altezza","mm","550","550"]
["","","","Larghezza","mm","765","765"]
["","","","Profondità","mm","285","285"]
["Peso","Unità","","","kg","41","41"]
["Motore del ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","500","500"]
["","","Riscaldamento","Bassissimo","giri/min","500","500"]
["Compressore","Type","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","48","48"]
["","Riscaldamento","","Alta","dBA","50","50"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carica","","","kg","1.15","1.15"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","0.78","0.8"]
["","GWP","","","","675","675.0"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","20"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 20m)","0,02 (per lunghezza delle tubazioni superiore ai 20m)"]
["","Dislivello","int. - est.","Max.","m","15.0","15.0"]
["","","int. - int.","Max.","m","7.5","7.5"]
["Attacchi tubazioni","Lunghezza totale delle tubazioni","Sistema","Reale","m","30","30"]
["Accessori standard","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentazione","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","220-230-240","220-230-240"]
["Note","","","","","(1) - Per un locale","(1) - Ogni unità D-AHU Daikin Professional può essere progettata secondo le tue esigenze. Seleziona la tua AHU su tools.daikinapplied.eu"]