{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B","4MXS80E3V3B2","4MXS80E7V3B"]
["Dimensioni","Unità","","Altezza","mm","770","770"]
["","","","Larghezza","mm","900","900"]
["","","","Profondità","mm","320","320"]
["Peso","Unità","","","kg","72","72"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Intervallo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","46","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-15","-15"]
["","","","Max.","°CBU","18","18"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","48","48"]
["","Riscaldamento","","Nom.","dBA","49","49"]
["Refrigerante","Tipo","","","","R-410A","R-410A"]
["","Charge","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Attacchi tubazioni","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 30m)","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Dislivello","int. - est.","Max.","m","15","15"]
["","","int. - int.","Max.","m","7.5","7.5"]
["","Lunghezza totale delle tubazioni","Sistema","Reale","m","70","70"]
["Accessori standard","Manuale di installazione","","","","1","1"]
["","Tappo di scarico","","","","1","1"]
["","Gruppo riduttore","","","","1","1"]
["Power supply","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","230","230"]
["Note","","","","","(1) - Raffreddamento: temp. interna 27°CBS, 19,0°CBU / temp. esterna 35°CBS; lunghezza equivalente delle tubazioni: 7,5m","(1) - Raffreddamento: temp. interna 27°CBS, 19,0°CBU / temp. esterna 35°CBS; lunghezza equivalente delle tubazioni: 7,5m"]
["","","","","","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 7,5m","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 7,5m"]
["","","","","","(3) - Contiene gas fluorurati a effetto serra","(3) - Contiene gas fluorurati a effetto serra"]
["Dimensioni","Unità","","Altezza","mm","","","770"]
["","","","Larghezza","mm","","","900"]
["","","","Profondità","mm","","","320"]
["Peso","Unità","","","kg","","","72"]
["Compressore","Tipo","","","","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","","","-10"]
["","","","Max.","°CBS","","","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","","","-15"]
["","","","Max.","°CBU","","","15.5"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","","","48"]
["","Riscaldamento","","Nom.","dBA","","","49"]
["Refrigerante","Tipo","","","","","","R-410A"]
["","Carica","","","kg","","","2.99"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","","25"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Dislivello","int. - est.","Max.","m","","","15"]
["","","int. - int.","Max.","m","","","7.5"]
["Attacchi tubazioni","Lunghezza totale delle tubazioni","Sistema","Reale","m","","","70"]
["Accessori standard","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Alimentazione","Fase","","","","","","1~"]
["","Frequenza","","","Hz","","","50"]
["","Tensione","","","V","","","230"]