{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Ventilatore","Portata d'aria","Raffrescamento","Bassissimo","m³/min","24.1"]
["","","Riscaldamento","Bassissimo","m³/min","24.1"]
["","","","Bassissimo","cfm","851"]
["","","Riscaldamento","Bassissimo","cfm","851"]
["Dimensioni","Unità","","Altezza","mm","734"]
["","","","Larghezza","mm","320"]
["","","","Profondità","mm","868"]
["Peso","Unità","","","kg","68"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10"]
["","","","Max.","°CBS","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-15"]
["","","","Max.","°CBU","18"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","52"]
["","Riscaldamento","","Nom.","dBA","52"]
["Refrigerante","Tipo","","","","R-32"]
["","Carica","","","kg","2.4"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","1.6"]
["","GWP","","","","675"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","25"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Dislivello","int. - est.","Max.","m","15"]
["","","int. - int.","Max.","m","7.5"]
["Attacchi tubazioni","Lunghezza totale delle tubazioni","Sistema","Reale","m","75"]
["Accessori standard","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Alimentazione","Fase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","220-240"]