{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Funzionamento silenzioso","dBA","","36","","41"]
["","","","Bassa","dBA","","38","","43"]
["","Raffrescamento","","Funzionamento silenzioso","dBA","","36","","41"]
["","","","Bassa","dBA","","38","","43"]
["","","","Alta","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Accessori standard","Manuale di installazione","","","","","Manuale di installazione","","Manuale di installazione"]
["","Manuale d’uso","","","","","Manuale d’uso","","Manuale d’uso"]
["","Viti","","","","","Viti","","Viti"]
["","Rondella","","","","","Rondella","","Rondella"]
["","Telecomando ad infrarossi","","","","","Telecomando ad infrarossi","","Telecomando ad infrarossi"]
["","Protezione griglia","","","","","Protezione griglia","","Protezione griglia"]
["","Batteria","","","","","Batteria","","Batteria"]
["Sistemi di controllo","Telecomando con cavo","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Attacchi tubazioni","Liquido","","DE","mm","","9.52","","9.52"]
["","Gas","","DE","mm","","15.88","","15.88"]
["","Scarico","","","","","19.05","","19.05"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","0.094","","0.137"]
["","Riscaldamento","","Nom.","kW","","0.094","","0.137"]
["Sound power level","Raffrescamento","","","dBA","","56","","60"]
["","Riscaldamento","","","dBA","","56","","60"]
["Dimensioni","Unità","","Larghezza","mm","","820","","820"]
["","","","Profondità","mm","","820","","820"]
["","","","Altezza","mm","","300","","300"]
["Rivestimento","Materiale","","","","","Acciaio zincato","","Acciaio zincato"]
["Peso","Unità","","","kg","","39","","39"]
["Ventilatore","Portata d'aria","Riscaldamento","Alta","m³/min","","29.2","","34.0"]
["","","","Bassa","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Raffrescamento","Bassa","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Alta","m³/min","","29.2","","34.0"]
["","","","Funzionamento silenzioso","m³/min","","17.6","","22.1"]
["","","Raffrescamento","Funzionamento silenzioso","m³/min","","17.6","","22.1"]
["Pannello decorativo","Peso","","","kg","","4","","4"]
["","Dimensioni","","Altezza","mm","","82","","82"]
["","","","Profondità","mm","","990","","990"]
["","","","Larghezza","mm","","990","","990"]
["","Colore","","","","","Bianco","","Bianco"]
["Power supply","Fase","","","","","1~","","1~"]
["","Nome","","","","","V1","","V1"]
["","Frequenza","","","Hz","","50","","50"]
["","Tensione","","","V","","220-240","","220-240"]
["Ventilatore","Portata d'aria","Riscaldamento","Funzionamento silenzioso","m³/min","15","","22.1"]
["Potenza assorbita","Riscaldamento","","Nom.","kW","0.067","","0.137"]
["","Raffrescamento","","Nom.","kW","0.067","","0.137"]
["Ventilatore","Portata d'aria","Raffrescamento","Funzionamento silenzioso","m³/min","15","","22.1"]
["Rivestimento","Materiale","","","","Acciaio zincato","","Acciaio zincato"]
["Dimensioni","Unità","","Altezza","mm","265","","300"]
["","","","Larghezza","mm","820","","820"]
["","","","Profondità","mm","820","","820"]
["Peso","Unità","","","kg","31","","39"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Bassa","m³/min","17.6","","26.3"]
["","","Riscaldamento","Alta","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Bassa","m³/min","17.6","","26.3"]
["Potenza sonora","Raffrescamento","","","dBA","54","","60"]
["","Riscaldamento","","","dBA","54","","60"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Bassa","dBA","35","","43"]
["","","","Funzionamento silenzioso","dBA","32","","41"]
["","Riscaldamento","","Alta","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Bassa","dBA","35","","43"]
["","","","Funzionamento silenzioso","dBA","32","","41"]
["Attacchi tubazioni","Liquido","","DE","mm","9.52","","9.52"]
["","Gas","","DE","mm","15.88","","15.88"]
["","Scarico","","","","19.05","","19.05"]
["Pannello decorativo","Dimensioni","","Altezza","mm","82","","82"]
["","","","Larghezza","mm","990","","990"]
["","","","Profondità","mm","990","","990"]
["","Peso","","","kg","4","","4"]
["Sistemi di controllo","Telecomando infrarossi","","","","ARCWLA","","ARCWLA"]
["","Telecomando con cavo","","","","ARCWB","","ARCWB"]
["Accessori standard","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Alimentazione","Fase","","","","1~","","1~"]
["","Frequenza","","","Hz","50","","50"]
["","Tensione","","","V","220-240","","220-240"]