{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L3"]
[]
[]
[]
[]
["","","","ADEQ35C2VEB / ARXS35L3V1B"]
["Capacità di raffrescamento","Nom.","kW","3.40 (1)"]
["Capacità di riscaldamento","Nom.","kW","4.00 (1)"]
["Note","","","(1) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale"]
["","","","(2) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["","","","(3) - PED: insieme = categoria l : non contemplata nella normativa PED ai sensi dell'articolo 1, punto 3.6 di 97/23/EC"]
["","","","(4) - Valore Ssc minimo (=potenza cortocircuito): Dispositivo conforme a EN 61000-3-2"]
["","","","(5) - Consultare i disegni separati per i dati elettrici"]
["","","","(6) - Contiene gas fluorurati a effetto serra"]