{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXC-D"]
[]
[]
[]
[]
["","","","","","ARXC20DV1B","ARXC25DV1B","ARXC35DV1B","ARXC50DV1B","ARXC60DV1B","ARXC71DV1B"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","45","46","51","54","54"]
["Refrigerante","GWP","","","","","675.0","675.0","675.0","675.0","675.0"]
["","Carica","","","kg","","0.550","0.750","1.00","1.10","1.15"]
["","Tipo","","","","","R-32","R-32","R-32","R-32","R-32"]
["Campo di funzionamento","Raffresc.","T. esterna","Max.","°CBS","","46","46","46","46","46"]
["","","","Min.","°CBS","","10","10","-10","-10","-10"]
["","Riscaldamento","T. esterna","Max.","°CBU","","18","18","18","18","18"]
["","","","Min.","°CBU","","-15","-15","-15","-15","-15"]
["Attacchi tubazioni","Dislivello","int. - est.","Max.","m","","15.0","15.0","20.0","20.0","20.0"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","0.017 (per lunghezza tubazioni superiore a 7,5m)","0.017 (per lunghezza tubazioni superiore a 7,5m)","0.017 (per lunghezza tubazioni superiore a 7,5m)","0.017 (per lunghezza tubazioni superiore a 7,5m)","0.017 (per lunghezza tubazioni superiore a 7,5m)"]
["Sound power level","Raffrescamento","","","dBA","","58","60","65","66","69"]
["Dimensioni","Unità","","Larghezza","mm","","658","658","845","845","930"]
["","","","Profondità","mm","","273","273","300","300","350"]
["","","","Altezza","mm","","550","550","615","615","695"]
["Compressore","Tipo","","","","","Swing ermetico","Swing ermetico","Swing ermetico","Swing ermetico","Swing ermetico"]
["Peso","Unità","","","kg","","24.0","26.0","39.0","39.0","45.0"]
["Power supply","Fase","","","","","1~","1~","1~","1~","1~"]
["","Frequenza","","","Hz","","50","50","50","50","50"]
["","Tensione","","","V","","220-240","220-240","220-240","220-240","220-240"]
["Potenza sonora","Raffrescamento","","","dBA","58"]
["Dimensioni","Unità","","Altezza","mm","550"]
["","","","Larghezza","mm","658"]
["","","","Profondità","mm","273"]
["Peso","Unità","","","kg","24"]
["Compressore","Tipo","","","","Swing ermetico"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","10"]
["","","","Max.","°CBS","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-15"]
["","","","Max.","°CBU","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","45"]
["Refrigerante","Tipo","","","","R-32"]
["","Carica","","","kg","0.55"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","0.371"]
["","GWP","","","","675.0"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","20"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0.017 (per lunghezza tubazioni superiore a 7,5m)"]
["","Dislivello","int. - est.","Max.","m","15.0"]
["Alimentazione","Fase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","220-240"]