{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","39.0","40.0","44.0"]
["","","","Medio","dBA","34.0","34.0","34.0"]
["","","","Funzionamento silenzioso","dBA","21.0","21.0","22.0"]
["","","","Bassa","dBA","28.0","28.0","28.0"]
["","Raffrescamento","","Medio","dBA","33.0","33.0","36.0"]
["","","","Funzionamento silenzioso","dBA","20.0","20.0","22.0"]
["","","","Bassa","dBA","25.0","26.0","30.0"]
["","","","Alta","dBA","39.0","40.0","45.0"]
["Accessori standard","Manuale di installazione","","","","1","1","1"]
["","Manuale d’uso","","","","1","1","1"]
["","Batterie","","","","1","1","1"]
["","Telecomando a raggi infrarossi","","","","1","1","1"]
["","Batterie a secco AAA","","","","2","2","2"]
["","Supporto del telecomando","","","","1","1","1"]
["","Piastra di montaggio","","","","1","1","1"]
["","Viti di fissaggio unità interna","","","","2","2","2"]
["Sistemi di comando","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Collegamenti tubazioni","Liquido","","DE","mm","6.35","6.35","6.35"]
["","Gas","","DE","mm","9.50","9.50","9.50"]
["","Scarico","","","","18","18","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.023","0.023","0.040"]
["","Riscaldamento","","Nom.","kW","0.023","0.023","0.040"]
["Sound power level","Raffrescamento","","","dBA","53.0","54.0","59.0"]
["","Riscaldamento","","","dBA","55.0","55.0","59.0"]
["Dimensioni","Unità","","Larghezza","mm","770","770","770"]
["","","","Profondità","mm","225","225","225"]
["","","","Altezza","mm","286","286","286"]
["Rivestimento","Colore","","","","Bianco","Bianco","Bianco"]
["Peso","Unità","","","kg","8.00","8.00","9.00"]
["Power supply","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","220-440","220-440","220-440"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","","","0.029"]
["","Riscaldamento","","Nom.","kW","","","","0.029"]
["Rivestimento","Colore","","","","","","","Bianco"]
["Dimensioni","Unità","","Altezza","mm","","","","286"]
["","","","Larghezza","mm","","","","770"]
["","","","Profondità","mm","","","","225"]
["Peso","Unità","","","kg","","","","8.5"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","","","11.8"]
["","","","Medio","m³/min","","","","8"]
["","","","Bassa","m³/min","","","","6.4"]
["","","","Funzionamento silenzioso","m³/min","","","","4.4"]
["","","Riscaldamento","Alta","m³/min","","","","11.9"]
["","","","Medio","m³/min","","","","8.6"]
["","","","Bassa","m³/min","","","","6.5"]
["","","","Funzionamento silenzioso","m³/min","","","","5.3"]
["Potenza sonora","Raffrescamento","","","dBA","","","","54"]
["","Riscaldamento","","","dBA","","","","56"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","","","43"]
["Pressione sonora","Raffrescamento","","Medio","dBA","","","","34"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","","","","27"]
["","","","Funzionamento silenzioso","dBA","","","","20"]
["","Riscaldamento","","Alta","dBA","","","","40"]
["Pressione sonora","Riscaldamento","","Medio","dBA","","","","35"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","","","","29"]
["","","","Funzionamento silenzioso","dBA","","","","21"]
["Attacchi tubazioni","Liquido","","DE","mm","","","","6.35"]
["","Gas","","DE","mm","","","","9.5"]
["","Scarico","","","","","","","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","","","","ARC470A1"]
["","Telecomando con cavo","","","","","","","BRC073A1"]
["Accessori standard","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Alimentazione","Fase","","","","","","","1~"]
["","Frequenza","","","Hz","","","","50"]
["","Tensione","","","V","","","","220-440"]