{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N / ARXM-R"]
[]
[]
[]
[]
["","","","","ATXM25N2V1B / ARXM25R5V1B","ATXM35N2V1B / ARXM35R5V1B"]
["Outdoor unit","","","","ARXM25R5V1B","ARXM35R5V1B"]
["Capacità di Raffrescamento","Min.","","kW","1.30","1.40"]
["","Capacità di Raffrescamento-=-Nom.-=-kW","","kW","2.50","3.40"]
["","Max.","","kW","3.20","4.00"]
["Capacità di riscaldamento","Min.","","kW","1.30","1.40"]
["","Nom.","","kW","2.80","4.00"]
["","Max.","","kW","4.70","5.20"]
["Efficienza nominale","EER","","","4.39","4.09"]
["","COP","","","5.00","4.04"]
["","Consumo energetico annuale","","kWh","285","416"]
["","Classe energetica","Raffreddamento","","A","A"]
["","","Riscaldamento","","A","A"]
["Raffrescamento ambienti","Classe di efficienza energetica","","","A+++","A+++"]
["","Capacità","Pdesign","kW","2.50","3.40"]
["","SEER","","","8.55","8.55"]
["","Consumi energetici annuali","","kWh/a","102","139"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Classe di efficienza energetica","","","A+++","A+++"]
["","Capacità","Pdesign","kW","2.40","2.50"]
["","SCOP/A","","","5.10","5.10"]
["","Pdh Capacità di riscaldamento a -10°","","kW","2.30","2.35"]
["","Consumi energetici annuali","","kWh/a","659","687"]
["Intervallo di efficienza energetica","","","","A+++ ~ D","A+++ ~ D"]