{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":70,"n_cols":9,"rows_kept":70,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXN-NB9"]
[]
[]
[]
[]
["","","","","","ATXN25NV1B9","ATXN35NV1B9","ATXN50NV1B9","ATXN60NV1B9"]
["Livello pressione sonora","Raffrescamento","","Funzionamento silenzioso","dBA","21","22","","33"]
["","","","Altissimo","dBA","41","42","","46"]
["","","","Bassa","dBA","29","30","","37"]
["","","","Alta","dBA","40","41","","43"]
["Accessori standard","Manuale di installazione","","","","1","1","","1"]
["","Manuale d’uso","","","","1","1","","1"]
["","Telecomando ad infrarossi","","","","1","1","","1"]
["","Batterie","","","","Batterie","Batterie","","Batterie"]
["","Supporto del telecomando","","","","1","1","","1"]
["","Piastra di montaggio","","","","1","1","","1"]
["","Filtri all'apatite di titanio","","","","Filtri all'apatite di titanio","Filtri all'apatite di titanio","","Filtri all'apatite di titanio"]
["Collegamenti tubazioni","Liquido","","DE","mm","6.35","6.35","","6.35"]
["","Gas","","DE","mm","9.50","9.50","","15.90"]
["","Scarico","","","","16.5","16.5","","16.5"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","693.00","1,060.00","","1,931.00"]
["","Riscaldamento","","Nom.","kW","700.00","950.00","","1,680.00"]
["Livello potenza sonora","Raffrescamento","","","dBA","53","54","","61"]
["Dimensioni","Unità","","Larghezza","mm","859","859","","1,124"]
["","","","Profondità","mm","209","209","","237"]
["","","","Altezza","mm","288","288","","310"]
["Rivestimento","Materiale","","","","Polistirene ad alto impatto","Polistirene ad alto impatto","","Polistirene ad alto impatto"]
["","Colore","","","","Bianco","Bianco","","Bianco"]
["Peso","Unità","","","kg","9.0","9.0","","14.0"]
["Power supply","Fase","","","","1~","1~","","1~"]
["","Frequenza","","","Hz","50","50","","50"]
["","Nome","","","","V1","V1","","V1"]
["","Tensione","","","V","220-240","220-240","","220-240"]
["Note","","","","","(1) - Tutte le unità sono state collaudate e sono conformi allo standard ISO5151 (unità non canalizzabili) o ISO13253 (unità canalizzabili)","(1) - Tutte le unità sono state collaudate e sono conformi allo standard ISO5151 (unità non canalizzabili) o ISO13253 (unità canalizzabili)","","(1) - Tutte le unità sono state collaudate e sono conformi allo standard ISO5151 (unità non canalizzabili) o ISO13253 (unità canalizzabili)"]
["","","","","","(2) - Tutte le specifiche sono soggette a modifiche senza preavviso da parte del costruttore.","(2) - Tutte le specifiche sono soggette a modifiche senza preavviso da parte del costruttore.","","(2) - Tutte le specifiche sono soggette a modifiche senza preavviso da parte del costruttore."]
["Ventilatore","Portata d'aria","Raffrescamento","Nom.","m³/min","","","13.30"]
["","","Riscaldamento","Nom.","m³/min","","","13.30"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","","1668"]
["","Riscaldamento","","Nom.","kW","","","1550"]
["Rivestimento","Colore","","","","","","Bianco"]
["","Materiale","","","","","","Polistirene ad alto impatto"]
["Dimensioni","Unità","","Altezza","mm","","","310"]
["","","","Larghezza","mm","","","1124"]
["","","","Profondità","mm","","","237"]
["Peso","Unità","","","kg","","","14"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","","15"]
["","","","Bassa","m³/min","","","11.8"]
["","","","Funzionamento silenzioso","m³/min","","","10.6"]
["","","Riscaldamento","Alta","m³/min","","","15.3"]
["","","","Bassa","m³/min","","","11.8"]
["","","","Funzionamento silenzioso","m³/min","","","10.6"]
["Potenza sonora","Raffrescamento","","","dBA","","","55"]
["Livello pressione sonora","Raffrescamento","","Altissimo","dBA","","","44"]
["","","","Alta","dBA","","","40"]
["","","","Bassa","dBA","","","35"]
["","","","Funzionamento silenzioso","dBA","","","32"]
["Attacchi tubazioni","Liquido","","DE","mm","","","6.35"]
["","Gas","","DE","mm","","","12.7"]
["","Scarico","","","","","","16.5"]
["Accessori standard","Installation manual","","","","","","1"]
["","Wireless remote control","","","","","","1"]
["","Titanium apatite filters","","","","","","Titanium apatite filters"]
["","Operation manual","","","","","","1"]
["","Batteries","","","","","","Batteries"]
["","Mounting plate","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Alimentazione","Nome","","","","","","V1"]
["","Fase","","","","","","1~"]
["","Frequenza","","","Hz","","","50"]
["","Tensione","","","V","","","220-240"]