{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXQ-A"]
[]
[]
[]
[]
["","","","","","ATXQ25AMV1B","ATXQ35AMV1B"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.023","0.025"]
["","Riscaldamento","","Nom.","kW","0.027","0.031"]
["Rivestimento","Colore","","","","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","291","291"]
["","","","Larghezza","mm","770","770"]
["","","","Profondità","mm","232","232"]
["Peso","Unità","","","kg","9","9"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","10.2","10.5"]
["","","","Medio","m³/min","8.1","8.5"]
["","","","Bassa","m³/min","6.5","7"]
["","","","Funzionamento silenzioso","m³/min","5","6"]
["","","Riscaldamento","Alta","m³/min","11.1","12"]
["","","","Medio","m³/min","9.6","10"]
["","","","Bassa","m³/min","8.1","8.3"]
["","","","Funzionamento silenzioso","m³/min","6.8","6.9"]
["Potenza sonora","Raffrescamento","","","dBA","55","55"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","40","41"]
["Pressione sonora","Raffrescamento","","Medio","dBA","34","35"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","26","28"]
["","","","Funzionamento silenzioso","dBA","23","24"]
["","Riscaldamento","","Alta","dBA","40","42"]
["Pressione sonora","Riscaldamento","","Medio","dBA","34","35"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","29","30"]
["","","","Funzionamento silenzioso","dBA","25","25"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35"]
["","Gas","","DE","mm","9.5","9.5"]
["","Scarico","","","","18","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","ARC470A1","ARC470A1"]
["Accessori standard","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Alimentazione","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","220-240","220-240"]