{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.029","0.029"]
["","Riscaldamento","","Nom.","kW","0.023","0.023"]
["Rivestimento","Colore","","","","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","295","295"]
["","","","Larghezza","mm","778","778"]
["","","","Profondità","mm","272","272"]
["Peso","Unità","","","kg","10","10"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","10.5","10.5"]
["","","","Medio","m³/min","7.5","7.5"]
["","","","Bassa","m³/min","5.7","5.7"]
["","","","Funzionamento silenzioso","m³/min","4.3","4.3"]
["","","Riscaldamento","Alta","m³/min","9.3","9.3"]
["","","","Medio","m³/min","8.2","8.2"]
["","","","Bassa","m³/min","6.2","6.2"]
["","","","Funzionamento silenzioso","m³/min","5.1","5.1"]
["Potenza sonora","Raffrescamento","","","dBA","57","57"]
["","Riscaldamento","","","dBA","54","54"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","41","41"]
["Pressione sonora","Raffrescamento","","Medio","dBA","33","33"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25","25"]
["","","","Funzionamento silenzioso","dBA","19","19"]
["","Riscaldamento","","Alta","dBA","39","39"]
["Pressione sonora","Riscaldamento","","Medio","dBA","34","34"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","26","26"]
["","","","Funzionamento silenzioso","dBA","20","20"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35"]
["","Gas","","DE","mm","9.5","9.5"]
["","Scarico","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC466A67","ARC466A67"]
["Sistemi di controllo","Telecomando con cavo","","","","BRC073A1","BRC073A1"]
["Accessori standard","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Alimentazione","Nome","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","220-240","220-240"]