{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","38","","41"]
["","","","Funzionamento silenzioso","dBA","21","","21"]
["","","","Bassa","dBA","28","","30"]
["","Raffrescamento","","Funzionamento silenzioso","dBA","21","","21"]
["","","","Bassa","dBA","25","","28"]
["","","","Alta","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Raffrescamento","","Nom.","dBA","31","","35"]
["Accessori standard","Manuale di installazione","","","","1","","1"]
["","Manuale d’uso","","","","1","","1"]
["","Telecomando ad infrarossi","","","","1","","1"]
["","Batterie","","","","2","","2"]
["","Supporto del telecomando","","","","1","","1"]
["","Piastra di montaggio","","","","1","","1"]
["","Viti di fissaggio unità interna","","","","2","","2"]
["","Filtro purificatore d'aria a base di apatite e titanio","","","","2","","2"]
["Sistemi di controllo","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Liquido","","DE","mm","6.35","","6.35"]
["","Gas","","DE","mm","9.5","","9.5"]
["","Scarico","","","","18","","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.040","","0.040"]
["","Riscaldamento","","Nom.","kW","0.040","","0.040"]
["Livello potenza sonora","Raffrescamento","","","dBA","55","","59"]
["","Riscaldamento","","","dBA","56","","58"]
["Dimensioni","Unità","","Larghezza","mm","780","","780"]
["","","","Profondità","mm","215","","215"]
["","","","Altezza","mm","289","","289"]
["Rivestimento","Colour","","","","Bianco","","Bianco"]
["Peso","Unità","","","kg","8","","8"]
["Ventilatore","Portata d'aria","Riscaldamento","Alta","m³/min","","","10.1"]
["","","","Bassa","m³/min","","","6.3"]
["","","","Funzionamento silenzioso","m³/min","","","4.3"]
["","","Raffrescamento","Bassa","m³/min","","","5.2"]
["","","","Alta","m³/min","","","9.2"]
["","","","Funzionamento silenzioso","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Raffrescamento","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Frequenza","","","Hz","50","","50"]
["","Nome","","","","V1","","V1"]
["","Tensione","","","V","220-240","","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","0.04","","0.040"]
["","Riscaldamento","","Nom.","kW","","0.04","","0.040"]
["Rivestimento","Colore","","","","","Bianco","","Bianco"]
["Dimensioni","Unità","","Altezza","mm","","289","","289"]
["","","","Larghezza","mm","","780","","780"]
["","","","Profondità","mm","","215","","215"]
["Peso","Unità","","","kg","","8","","8.00"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","7.9","","9.2"]
["","","","Medio","m³/min","","6.3","","7.2"]
["","","","Bassa","m³/min","","4.7","","5.2"]
["","","","Funzionamento silenzioso","m³/min","","3.9","","3.9"]
["","","Riscaldamento","Alta","m³/min","","9","","10.1"]
["","","","Medio","m³/min","","7.5","","8.1"]
["","","","Bassa","m³/min","","6","","6.3"]
["","","","Funzionamento silenzioso","m³/min","","4.3","","4.3"]
["Potenza sonora","Raffrescamento","","","dBA","","55","","59"]
["","Riscaldamento","","","dBA","","56","","58"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","37","","42"]
["Pressione sonora","Raffrescamento","","Medio","dBA","","31","","35"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","","25","","28"]
["","","","Funzionamento silenzioso","dBA","","21","","21"]
["","Riscaldamento","","Alta","dBA","","38","","41"]
["Pressione sonora","Riscaldamento","","Medio","dBA","","33","","36"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","","28","","30"]
["","","","Funzionamento silenzioso","dBA","","21","","21"]
["Attacchi tubazioni","Liquido","","DE","mm","","6.35","","6.35"]
["","Gas","","DE","mm","","9.5","","9.50"]
["","Scarico","","","","","18","","18"]
["Sistemi di controllo","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Accessori standard","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Alimentazione","Nome","","","","","V1","","V1"]
["","Fase","","","","","1~","","1~"]
["","Frequenza","","","Hz","","50","","50"]
["","Tensione","","","V","","220-240","","220-240"]