{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM601A51"]
[]
[]
[]
[]
["","","","","DCM601A51."]
["Temperatura esterna","Umidità relativa <","","%","85"]
["Massimo numero di unità interne collegabili","","","","64, 512 (1), 2,560 (2)"]
["Potenza assorbita","kW","","","0.023"]
["Comunicazione","DIII-NET","Quantità","","1"]
["","Ethernet","Nota","","Accesso web (100BASE-TX)"]
["","","Quantità","","1"]
["","Modem","Nota","","Sistema di manutenzione della rete di climatizzazione (Air Conditioning Network Service System)"]
["Installazione","","","","Solo direzione verticale"]
["Dimensioni","Unità","Larghezza","mm","290"]
["","","Profondità","mm","50"]
["","","Altezza","mm","243"]
["Peso","Unità","","kg","2.4"]
["Power supply","Frequenza","","Hz","50/60"]
["","Tensione","","V","AC 100-240"]
["Note","","","","(1) - Con 7 ITM più adattatori"]
["","","","","(2) - Con 5 ITM combinati con ITM integrator"]