{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3"]
[]
[]
[]
[]
["","","","","","EHSHB04P30DA3","EHSHB08P30DA3","EHSHB08P50DA3"]
["Rivestimento","Colore","","","","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)"]
["","Materiale","","","","Polipropilene resistente agli urti","Polipropilene resistente agli urti","Polipropilene resistente agli urti"]
["Dimensioni","Unità","","Altezza","mm","1891","1891","1896"]
["","","","Larghezza","mm","595","595","790"]
["","","","Profondità","mm","615","615","790"]
["Peso","Unità","","","kg","76.0","76.0","99.0"]
["PED","Categoria","","","","art. 3.3","art. 3.3","art. 3.3"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Carica","","","kg","1.50","1.50","1.50"]
["Livello potenza sonora","Nom.","","","dBA","39","39","39"]
["Campo di funzionamento","Riscaldamento","Lato acqua","Min.","°C","18","18","18"]
["","","","Max.","°C","65","65","65"]
["","Raffrescamento","T. esterna","Min.","°CBS","10","10","10"]
["","","Lato acqua","Min.","°C","5","5","5"]
["","","","Max.","°C","22","22","22"]
["Alimentazione","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","230","230","230"]
["Riscaldatore elettrico","Alimentazione","","Nome","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frequenza","Hz","50","50","50"]
["Note","","","","","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","","","(5) - Riscaldamento del serbatoio solo con pompa di calore, senza riscaldatore elettrico"]