{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EJHA-AV3"]
[]
[]
[]
[]
["","","","","","EJHA04AAV3"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","37.0"]
["Refrigerante","GWP","","","","675.0"]
["","Carica","","","kg","0.560"]
["","Tipo","","","","R-32"]
["Campo di funzionamento","Riscaldamento","T. esterna","Max.","°CBU","25"]
["","Acqua calda sanitaria","T. esterna","Min.","°CBS","-14"]
["","","","Max.","°CBS","35"]
["Potenza assorbita","Riscaldamento","","Nom.","kW","0.850 (1)"]
["Sound power level","Heating","","Nom.","dBA","58.7"]
["COP","","","","","4.49 (1)"]
["Dimensioni","Unità","","Larghezza","mm","845"]
["","","","Profondità","mm","329"]
["","","","Altezza","mm","745"]
["Peso","Unità","","","kg","45.0"]
["Risc. amb.","Uscita acqua cond. clim. medie 35°C","Generale","ηs (Efficienza stagionale Risc. amb.)","%","116"]
["","","","Classe efficienza stagionale Risc. amb.","","A"]
["","","","SCOP","","2.98"]
["","Uscita acqua cond. clim. medie 55°C","Generale","Seasonal space heating eff. class","","A+"]
["","","","ηs (Efficienza stagionale Risc. amb.)","%","101"]
["","","","SCOP","","2.60"]
["Ventilatore","Portata d'aria","Riscaldamento","Alta","m³/min","28.3"]
["Capacità di riscaldamento","Nom.","","","kW","4.53 (1)"]
["Power supply","Fase","","","","1~"]
["","Nome","","","","V3"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","220-240"]
["Note","","","","","(1) - Riscaldamento: temp. acqua in uscita condensatore 35°C; Dt 5°C; temperatura dell'aria esterna 7°CBS, 6°CBU"]