{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHP-A2V3"]
[]
[]
[]
[]
["","","","","EKHHP300AC2V3","EKHHP500AC2V3","EKHHP300AA2V3 (Archived)","EKHHP300AB2V3 (Archived)","EKHHP500AB2V3 (Archived)","EKHHP500AA2V3 (Archived)"]
["Livello pressione sonora","Nom.","","dBA","0","0","0","0","0","0"]
["Refrigerante","GWP","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Tipo","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Potenza sonora","Nom.","","dBA","39","39","0","39","39","0"]
["Dimensioni","Unità","Larghezza","mm","595","790","615","595","790","790"]
["","","Profondità","mm","615","790","615","615","790","790"]
["","","Altezza","mm","1,772","1,778","1,750","1,772","1,778","1,750"]
["Rivestimento","Colore","","","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)"]
["PED","Categoria","","","Categoria I","Categoria I","Categoria I","Categoria I","Categoria I","Categoria I"]
["Peso","Unità","","kg","70","80","70","70","80","80"]
["Power supply","Fase","","","1~","1~","3N~","1~","1~","3N~"]
["","Frequenza","","Hz","50","50","50","50","50","50"]
["","Tensione","","V","230","230","230","230","230","230"]
["Corrente","Fusibili consigliati","","A","16","16","16","16","16","16"]
["Note","","","","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897"]