{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-PB"]
[]
[]
[]
[]
["","","","","","EKHWP300PB","EKHWP500PB"]
["Montaggio","","","","","Pavimento","Pavimento"]
["Rivestimento","Colore","","","","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)"]
["","Materiale","","","","Polipropilene resistente agli urti","Polipropilene resistente agli urti"]
["Dimensioni","Unità","Altezza","Serbatoio","mm","1646","1658"]
["","","","Larghezza","mm","595","790"]
["","","","Profondità","mm","615","790"]
["Peso","Unità","","Vuoto","kg","56","82"]
["","","","Piena","kg","350","559"]
["Serbatoio","Volume acqua","","","l","294","477"]
["","Materiale","","","","Polipropilene","Polipropilene"]
["","Max. temperatura acqua","","","°C","85","85"]
["","Classe di efficienza energetica","","","","B","B"]
["Scambiatore di calore","Acqua calda sanitaria","","Quantità","","1","1"]
["","","","Materiale tubo","","Acciaio inox (DIN 1.4404)","Acciaio inox (DIN 1.4404)"]
["","","","Volume batteria interna","l","27.8","29.0"]
["","","","Pressione d'esercizio","bar","10.0","10.0"]
["","Carica","","Quantità","","1","1"]
["","","","Materiale tubo","","Acciaio inox (DIN 1.4404)","Acciaio inox (DIN 1.4404)"]
["","","","Volume batteria interna","l","12.9","18.1"]
["","","","Pressione d'esercizio","bar","6.0","6.0"]
["","Riscaldamento solare ausiliario","","Quantità","","","1"]
["","","","Materiale tubo","","","Acciaio inox (DIN 1.4404)"]
["","","","Volume batteria interna","l","","3.9"]
["","","","Pressione d'esercizio","bar","","3.0"]
["Note","","","","","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - Per volume utilizzato 140l -> 5820 Wh (vasca) / 8kW pompa di calore","(5) - Per volume utilizzato 140l -> 5820 Wh (vasca) / 16kW pompa di calore"]
["","","","","","(6) - Per volume utilizzato 90l -> 3660 Wh (vasca) / 8kW pompa di calore","(6) - Per volume utilizzato 90l -> 3660 Wh (vasca) / 16kW pompa di calore"]