{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMB-AH"]
[]
[]
[]
[]
["","","","","","EKOMB22AAV1H","EKOMB28AAV1H","EKOMB33AAV1H"]
["Acqua calda sanitaria","Assorbimento di calore (valore calorifico lordo) Qnw","Nom.","Max","kW","24.6","31.1","36.3"]
["","","","Min","kW","6.2","7.9","8.0"]
["","Classe di comfort (EN13203)","","","","L","XL","XL"]
["","Temperatura","","Max","°C","65","65","65"]
["","Assorbimento di calore (valore calorifico netto) Qnw","Nom.","Min","kW","5.6","7.1","7.2"]
["","","","Max","kW","22.1","28.0","32.7"]
["Gas combustibile","Temperatura","","Max","°C","90","90","90"]
["","Portata (G31)","","Max","kg/h","36.4","46.1","54.4"]
["Aria di immissione","Concentrico","","","","60/100","60/100","60/100"]
["Riscaldamento acqua calda sanitaria","Generale","","Classe di efficienza energetica riscaldamento acqua","","A","A","A"]
["","","","Profilo di carico dichiarato","","L","XL","XL"]
["Dimensioni","Unità","Altezza","Struttura","mm","590","650","710"]
["Rivestimento","Materiale","","","","Piastra di lamiera rivestita","Piastra di lamiera rivestita","Piastra di lamiera rivestita"]
["","Colore","","","","RAL9010","RAL9010","RAL9010"]
["Risc. amb.","Generale","","Classe efficienza stagionale riscaldamento ambienti","","A","A","A"]
["","","","ηs (Efficienza stagionale riscaldamento ambienti)","%","91","92","93"]
["Riscaldamento centrale","Assorbimento di calore Qn (valore calorifico lordo)","Nom.","Min","kW","6.2","7.9","8.0"]
["","","","Max","kW","20.8","26.3","30.3"]
["","Temperatura acqua","","Max","°C","90","90","90"]
["","Pn in uscita a 80/60°C","","Nom.","kW","17.8","22.8","26.3"]
["","Assorbimento di calore Qn (valore calorifico netto)","Nom.","Max","kW","18.7","23.7","27.3"]
["","","","Min","kW","5.6","7.1","7.2"]
["Gas","Attacco","","Diametro","mm","15","15","15"]
["","Consumi (G31)","","Min","m³/ora","0.22","0.28","0.28"]
["","","","Max","m³/ora","0.87","1.11","1.29"]
["","Classe NOx","","","","6","6","6"]