{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTW"]
[]
[]
[]
[]
["","","","","EKRTWA"]
["Funzione di regolazione","","","","Banda proporzionale"]
["Dimensioni","Unità","Larghezza","mm","125"]
["","","Profondità","mm","34"]
["","","Altezza","mm","87"]
["Intervallo di temperatura impostato","Riscaldamento","Max.","°C","37"]
["","","Min.","°C","4"]
["","Raffrescamento","Max.","°C","37"]
["","","Min.","°C","4"]
["Orologio","","","","Sì"]
["Peso","Unità","","g","215"]
["Temperatura esterna","Magazzinamento","Min.","°C","-20"]
["","","Max.","°F","140"]
["","","Min.","°F","-4"]
["","","Max.","°C","60"]
["","Funzionamento","Min.","°C","0"]
["","","Max.","°F","122"]
["","","Min.","°F","32"]
["","","Max.","°C","50"]
["Massima corrente di interruzione nominale (a 230VCA)","A","","","5.0 (1)"]
["Collegamento","Tipo","","","A filo"]
["Power supply","Tensione","","V","A batterie 3* AA-LR6 (alcaline)"]
["Note","","","","(1) - 230VCA"]