{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Dimensioni","Unità","","Altezza","mm","870","870"]
["","","","Larghezza","mm","1100","1100"]
["","","","Profondità","mm","460","460"]
["Peso","Unità","","","kg","101","101"]
["Ventilatore","Portata d'aria","Riscaldamento","Alta","m³/min","85.0","85.0"]
["","","Raffrescamento","Alta","m³/min","85","85"]
["Campo di funz.","Raffresc.","","Min.","°CBS","10","10"]
["","","","Max.","°CBS","43","43"]
["Campo di funzionamento","Acqua calda sanitaria","","Min.","°CBS","-25","-25"]
["Campo di funz.","Acqua calda sanitaria","","Max.","°CBS","25 (1), 35 (1)","25 (1), 35 (1)"]
["Livello potenza sonora","Riscaldamento","","Nom.","dBA","62.0 (2)","62.0 (2)"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","48.0 (2)","48.0 (2)"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","2.57","2.57"]
["","Carica","","","kg","3.8","3.8"]
["Attacchi tubazioni","Liquido","","DE","mm","9.5","9.5"]
["","Gas","","DE","mm","15.9","15.9"]
["Collegamenti tubazioni","Scarico","","DE","mm","26","26"]
["","Dislivello","int. - est.","Max.","m","30.0","30.0"]
["Attacchi tubazioni","Isolamento termico","","","","Sulla linea del liquido e su quella del gas","Sulla linea del liquido e su quella del gas"]
["Alimentazione","Nome","","","","W1","W1"]
["","Fase","","","","3~","3~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","400","400"]
["Corrente","Fusibili consigliati","","","A","16","16"]
["Note","","","","","(1) - Per maggiori dettagli, vedere i disegni relativi al campo di funzionamento","(1) - Per maggiori dettagli, vedere i disegni relativi al campo di funzionamento"]
["","","","","","(2) - Misurato con perdita di carico di 10 kPa nel sistema di riscaldamento a condizioni di funzionamento dell’acqua in uscita di 47-55°C in un ambiente con temperatura esterna di 20°C. BS/BU 7°C/6°.","(2) - Misurato con perdita di carico di 10 kPa nel sistema di riscaldamento a condizioni di funzionamento dell’acqua in uscita di 47-55°C in un ambiente con temperatura esterna di 20°C. BS/BU 7°C/6°."]