{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH-D"]
[]
[]
[]
[]
["","","","","","ETSH16P30DA","ETSH16P50DA"]
["Livello pressione sonora","Nom.","","","dBA","32.8","32.8"]
["Campo di funzionamento","Raffresc.","T. esterna","Min.","°CBS","10","10"]
["","","Lato acqua","Max.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Heating","Lato acqua","Max.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Livello potenza sonora","Nom.","","","dBA","45.6","45.6"]
["Dimensioni","Unità","","Larghezza","mm","590","785"]
["","","","Profondità","mm","615","785"]
["","","","Altezza","mm","1,891","1,896"]
["Rivestimento","Materiale","","","","Polipropilene resistente agli urti","Polipropilene resistente agli urti"]
["","Colour","","","","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)","Bianco traffico (RAL9016) / Grigio scuro (RAL7011)"]
["PED","Categoria","","","","Art4.3","Art4.3"]
["Peso","Unità","","","kg","73","90"]
["Power supply","Phase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","230","230"]
["Riscaldatore elettrico","Alimentazione","","Frequenza","Hz","50","50"]
["","","","Nome","","3V / 9W","3V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~"]
["Note","","","","","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]