{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH16E"]
[]
[]
[]
[]
["","","","","","ETSH16P30EF","ETSH16P50EF"]
["Rivestimento","Colore","","","","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)"]
["","Materiale","","","","Polipropilene resistente agli urti","Polipropilene resistente agli urti"]
["Dimensioni","Unità","","Altezza","mm","1,892","1,910"]
["","","","Larghezza","mm","594","792"]
["","","","Profondità","mm","644","816"]
["Peso","Unità","","","kg","75","98"]
["Sound power level","Nom.","","","dBA","45.6","45.6"]
["Livello pressione sonora","Nom.","","","dBA","32.8","32.8"]
["Campo di funzionamento","Riscaldamento","Lato acqua","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["","Raffresc.","T. esterna","Min.","°CBS","0 (2)","0 (2)"]
["","","Lato acqua","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["Power supply","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","230","230"]
["Note","","","","","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897"]
["","","","","","(2) - Fare riferimento ai disegni relativi ai limiti di funzionamento","(2) - Fare riferimento ai disegni relativi ai limiti di funzionamento"]