{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Rivestimento","Colore","","","","Bianco","Bianco"]
["","Materiale","","","","Resina","Resina"]
["Dimensioni","Unità","","Altezza","mm","290","340"]
["","","","Larghezza","mm","1050","1200"]
["","","","Profondità","mm","269","262"]
["Peso","Unità","","","kg","14","18"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","16.2","23"]
["","","","Medio","m³/min","13.4","21.1"]
["","","","Bassa","m³/min","12.1","18.7"]
["","","Riscaldamento","Alta","m³/min","16.9","23"]
["","","","Medio","m³/min","14.2","20.9"]
["","","","Bassa","m³/min","12.7","18.7"]
["Potenza sonora","Raffrescamento","","","dBA","61","65"]
["","Riscaldamento","","","dBA","61","65"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","45","49"]
["Pressione sonora","Raffrescamento","","Medio","dBA","42","45"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","40","41"]
["","Riscaldamento","","Alta","dBA","45","49"]
["Pressione sonora","Riscaldamento","","Medio","dBA","42","45"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","40","41"]
["Attacchi tubazioni","Liquido","","DE","mm","9.52","9.52"]
["","Gas","","DE","mm","15.9","15.9"]
["","Scarico","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Alimentazione","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","220-240","220-240"]
["Accessori standard","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Note","","","","","(1) - Le capacità di raffrescamento nom. si riferiscono a: temperatura interna: 27°CBS, 19°CBU, temperatura esterna: 35°CBS, lunghezza equivalente delle tubazioni del refrigerante: 5m, dislivello: 0m."]
["","","","","","(2) - Le capacità di riscaldamento nominali si riferiscono a: temperatura interna: 20°CBS, temperatura esterna: 7°CBS, 6°CBU, lunghezza equivalente delle tubazioni: 5m, dislivello: 0m."]
["Accessori standard","Screw cover","","","","","3"]