{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / FBQ35C8VEB / RZQG71L9V1B","FBQ71C8VEB / RZQG71L9V1B","FBQ100C8VEB / RZQG100L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / RZQG100L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG125L9V1B","FBQ125C8VEB / RZQG125L9V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQG125L9V1B","FBQ60C8VEB / FBQ60C8VEB / RZQG125L9V1B"]
["Capacità di Raffrescamento","Nom.","","kW","","6.8","9.5","","","","12.0"]
["Raffrescamento ambienti","SEER","","","5.10","5.61, 6.11","5.80","5.10","5.10","5.10","5.81","5.10","5.10"]
["","Consumi energetici annuali","","kWh/a","467","390","574","652","652","824","723","824","824"]
["","Capacità","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Classe di efficienza energetica","","","B","A++","A+","B","B","B","A+","B","B"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","6.00","6.00","11.30","11.30","11.30","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","3.80","4.01","4.61","3.80","3.80","3.80","4.21","3.80","3.80"]
["","Classe di efficienza energetica","","","A","A+","A++","A","A","A","A+","A","A"]
["","Consumi energetici annuali","","kWh/a","2,211","2,095","3,432","4,164","4,164","4,683","4,227","4,683","4,683"]
["Efficienza nominale","Consumo energetico annuale","","kWh","","970","1,220","","","","1,575"]
["","EER","","","","3.50","3.89","","","","3.81"]
["","COP","","","","3.65","4.21","","","","3.83"]
["","Classe energetica","Raffreddamento","","","A","A","","","","A"]
["","","Riscaldamento","","","A","A","","","","A"]
["Capacità di riscaldamento","Nom.","","kW","","7.5","10.8","","","","13.5"]
["Note","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["","","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["","","","","","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale","","","","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale"]