{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / ARXM-N9"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / ARXM71N2V1B9"]
["Capacità di raffrescamento","Max.","","kW","7.05"]
["","Nom.","","kW","6.80"]
["Efficienza nominale","Consumo energetico annuale","","kWh","1,083"]
["","EER","","","3.14"]
["","COP","","","3.38"]
["","Classe energetica","Raffreddamento","","B"]
["","","Riscaldamento","","C"]
["Capacità di riscaldamento","Nom.","","kW","7.50"]
["","Max.","","kW","7.58"]
["Note","","","","(1) - Per informazioni sul campo di funzionamento consultare i disegni separati"]
["","","","","(2) - Consultare i disegni separati per i dati elettrici"]
["","","","","(3) - Le capacità di raffrescamento nom. si riferiscono a: temperatura interna: 27°CBS, 19°CBU, temperatura esterna: 35°CBS, lunghezza equivalente delle tubazioni del refrigerante: 5m, dislivello: 0m."]
["","","","","(4) - Le capacità di riscaldamento nominali si riferiscono a: temperatura interna: 20°CBS, temperatura esterna: 7°CBS, 6°CBU, lunghezza equivalente delle tubazioni: 5m, dislivello: 0m."]