{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":12,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B"]
[]
[]
[]
[]
["","","","","","FCAG35BVEB","FCAG50BVEB","FCAG60BVEB","FCAG71BVEB","FCAG100BVEB","FCAG125BVEB","FCAG140BVEB"]
["Capacità di Raffrescamento","Capacità totale","","Nom.","kW","3.50","5.00","5.70","6.80","9.5","12.1","13.40"]
["Capacità di riscaldamento","Capacità totale","","Nom.","kW","4.2","6.0","7.0","7.5","10.8","13.5","15.5"]
["Rivestimento","Materiale","","","","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato"]
["Dimensioni","Unità","","Altezza","mm","204","204","204","204","246","246","246"]
["","","","Larghezza","mm","840","840","840","840","840","840","840"]
["","","","Profondità","mm","840","840","840","840","840","840","840"]
["Peso","Unità","","","kg","18","19","19","21","23","23","23"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","12.9","14.6","14.9","15.1","22.7","27.2","27.2"]
["","","","Medio","m³/min","10.6","11.8","12.2","13","17.8","20.4","20.4"]
["","","","Bassa","m³/min","8.8","9.4","9.6","10.8","13","13.1","13.1"]
["","","Riscaldamento","Alta","m³/min","14.1","14.6","14.9","15.1","23","27","27"]
["","","","Medio","m³/min","11.6","11.8","12.2","12.9","18.1","20.2","20.2"]
["","","","Bassa","m³/min","9.4","9.4","9.6","10.8","13.2","13","13"]
["Potenza sonora","Raffrescamento","","","dBA","49","49","51","51","54","58","58"]
["","Riscaldamento","","","dBA","49","49","51","51","54","58","58"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","31","31","33","35","37","41","41"]
["Pressione sonora","Raffrescamento","","Medio","dBA","29","29","31","31","33","35","35"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","27","27","28","28","29","29","29"]
["","Riscaldamento","","Alta","dBA","31","31","33","33","37","41","41"]
["Pressione sonora","Riscaldamento","","Medio","dBA","29","29","31","31","33","35","35"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","27","27","28","28","29","29","29"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gas","","DE","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Scarico","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Pannello decorativo","Modello","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Dimensioni","","Altezza","mm","65","65","65","65","65","65","65"]
["","","","Larghezza","mm","950","950","950","950","950","950","950"]
["","","","Profondità","mm","950","950","950","950","950","950","950"]
["","Peso","","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["Pannello decorativo 2","Modello","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Dimensioni","","Altezza","mm","148","148","148","148","148","148","148"]
["","","","Larghezza","mm","950","950","950","950","950","950","950"]
["","","","Profondità","mm","950","950","950","950","950","950","950"]
["","Peso","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["Pannello decorativo 3","Modello","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Dimensioni","","Altezza","mm","106","106","106","106","106","106","106"]
["","","","Larghezza","mm","950","950","950","950","950","950","950"]
["","","","Profondità","mm","950","950","950","950","950","950","950"]
["","Peso","","","kg","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["Sistemi di comando","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["Sistemi di controllo","Telecomando con cavo","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7"]
["Accessori standard","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1"]
["Alimentazione","Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Alimentazione-=-Frequenza","","Frequenza","","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Alimentazione-=-Tensione","","Tensione","","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Sistemi di controllo","Telecomando infrarossi","","","","","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]