{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQG71L8Y1B","FCQHG71FVEB / RZQG71L8Y1B","FCQHG140FVEB / RZQG100L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG100L8Y1B","FCQHG140FVEB / RZQG125L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG125L8Y1B","FCQHG140FVEB / RZQG140L7Y1B"]
["Capacità di raffrescamento","Nom.","","kW","","6.80","","","","","13.4"]
["Raffrescamento ambienti","SEER","","","7.00","6.91","7.00","5.10","6.61","5.10"]
["","Consumi energetici annuali","","kWh/a","340","345","475","652","636","824"]
["","Capacità","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Classe di efficienza energetica","","","A++","A++","A++","B","A++","B"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","7.60","7.60","11.30","11.30","12.66","12.71"]
["","SCOP/A","","","4.54","4.54","4.80","3.80","4.63","3.80"]
["","Classe di efficienza energetica","","","A+","A+","A++","A","A++","A"]
["","Consumi energetici annuali","","kWh/a","2,344","2,344","3,296","4,164","3,829","4,683"]
["Efficienza nominale","Consumo energetico annuale","","kWh","","830"]
["","EER","","","","4.09","","","","","3.35"]
["","COP","","","","4.80","","","","","4.12"]
["","Classe energetica","Raffreddamento","","","A"]
["","","Riscaldamento","","","A"]
["Capacità di riscaldamento","Nom.","","kW","","7.5","","","","","15.5"]
["Note","","","","","(1) - Il consumo energetico annuale è conforme alla direttiva 2002/31/CE sulla classificazione energetica","","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["","","","","","(2) - I valori SEER e SCOP sono conformi alla norma europea EN 14825","","","","","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale"]