{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","35","35","38","38"]
["","","Medio","dBA","33","33","35","35"]
["","","Bassa","dBA","27","27","30","30"]
["","Raffrescamento","Medio","dBA","33","33","35","35"]
["","","Bassa","dBA","27","27","30","30"]
["","","Alta","dBA","35","35","38","38"]
["Accessori standard","Manuale di installazione","","","1","1","1","1"]
["","Manuale d’uso","","","1","1","1","1"]
["","Isolante per il collegamento","","","1","1","1","1"]
["","Materiale di tenuta","","","1","1","1","1"]
["","Fascetta metallica","","","1","1","1","1"]
["","Tubo flessibile di scarico","","","1","1","1","1"]
["","Rondella per staffa di sospensione","","","8","8","8","8"]
["","Materiale sigillante","","","2","2","2","2"]
["","Fascette","","","6","6","6","6"]
["","Piastra di fissaggio rondella","","","4","4","4","4"]
["","Viti per flange canalizzazione","","","1","1","1","1"]
["","Filtro aria","","","1","1","1","1"]
["Attacchi tubazioni","Liquido","DE","mm","6.35","6.35","6.35","6.35"]
["","Gas","DE","mm","9.50","9.50","12.70","12.70"]
["","Scarico","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Potenza assorbita","Raffrescamento","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Riscaldamento","Nom.","kW","0.036","0.036","0.060","0.060"]
["Potenza sonora","Raffrescamento","","dBA","53","53","55","56"]
["","Riscaldamento","","dBA","53","53","55","56"]
["Dimensioni","Unità","Larghezza","mm","750","750","1,150","1,150"]
["","","Profondità","mm","620","620","620","620"]
["","","Altezza","mm","200","200","200","200"]
["Peso","Unità","","kg","21","21","28","28"]
["Ventilatore","Pressione statica esterna","Nom.","Pa","30","30","40","40"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frequenza","","Hz","50","50","50","50"]
["","Tensione","","V","220-240","220-240","220-240","220-240"]