{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","35.0","35.0","","38.0"]
["","","","Medio","dBA","33.0","33.0","","35.0"]
["","","","Bassa","dBA","27.0","27.0","","30.0"]
["","Raffrescamento","","Medio","dBA","33.0","33.0","","35.0"]
["","","","Bassa","dBA","27.0","27.0","","30.0"]
["","","","Alta","dBA","35.0","35.0","","38.0"]
["Accessori standard","Manuale di installazione","","","","1","1","","1"]
["","Manuale d’uso","","","","1","1","","1"]
["","Isolante per il collegamento","","","","1","1","","1"]
["","Materiale di tenuta","","","","1","1","","1"]
["","Fascetta metallica","","","","1","1","","1"]
["","Tubo flessibile di scarico","","","","1","1","","1"]
["","Rondella per staffa di sospensione","","","","8","8","","8"]
["","Materiale sigillante","","","","2","2","","2"]
["","Fascette","","","","6","6","","6"]
["","Piastra di fissaggio rondella","","","","4","4","","4"]
["","Viti per flange canalizzazione","","","","1","1","","1"]
["","Filtro aria","","","","1","1","","1"]
["Collegamenti tubazioni","Liquido","","DE","mm","6.35","6.35","","6.35"]
["","Gas","","DE","mm","9.50","9.50","","12.70"]
["","Scarico","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.036","0.036","","0.060"]
["","Riscaldamento","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Raffrescamento","","","dBA","53.0","53.0","","56.0"]
["","Riscaldamento","","","dBA","53.0","53.0","","56.0"]
["Dimensioni","Unità","","Larghezza","mm","750","750","","1,150"]
["","","","Profondità","mm","620","620","","620"]
["","","","Altezza","mm","200","200","","200"]
["Peso","Unità","","","kg","21","21","","28"]
["Ventilatore","Prevalenza","","Nom.","Pa","30","30","","40"]
["","Portata d'aria","Riscaldamento","Alta","m³/min","8.7","8.7","","16.0"]
["","","","Medio","m³/min","8.0","8.0","","14.8"]
["","","","Bassa","m³/min","7.3","7.3","","13.5"]
["","","Raffrescamento","Bassa","m³/min","7.3","7.3","","13.5"]
["","","","Medio","m³/min","8.0","8.0","","14.8"]
["","","","Alta","m³/min","8.7","8.7","","16.0"]
["Power supply","Fase","","","","1~","1~","","1~"]
["","Frequenza","","","Hz","50","50","","50"]
["","Tensione","","","V","220-240","220-240","","220-240"]
["Note","","","","","(1) - Consultare i disegni separati per i dati elettrici","(1) - Consultare i disegni separati per i dati elettrici","","(1) - Consultare i disegni separati per i dati elettrici"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","","0.060"]
["","Riscaldamento","","Nom.","kW","","","0.060"]
["Dimensioni","Unità","","Altezza","mm","","","200"]
["","","","Larghezza","mm","","","1150"]
["","","","Profondità","mm","","","620"]
["Peso","Unità","","","kg","","","28"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","","15.8"]
["","","","Medio","m³/min","","","14.6"]
["","","","Bassa","m³/min","","","13.3"]
["","","Riscaldamento","Alta","m³/min","","","15.8"]
["","","","Medio","m³/min","","","14.6"]
["","","","Bassa","m³/min","","","13.3"]
["","Prevalenza","","Nom.","Pa","","","40"]
["Potenza sonora","Raffrescamento","","","dBA","","","55.0"]
["","Riscaldamento","","","dBA","","","55.0"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","","38.0"]
["Pressione sonora","Raffrescamento","","Medio","dBA","","","35.0"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","","","30.0"]
["","Riscaldamento","","Alta","dBA","","","38.0"]
["Pressione sonora","Riscaldamento","","Medio","dBA","","","35.0"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","","","30.0"]
["Attacchi tubazioni","Liquido","","DE","mm","","","6.35"]
["","Gas","","DE","mm","","","12.70"]
["","Scarico","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Accessori standard","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Filtro aria","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Alimentazione","Fase","","","","","","1~"]
["","Frequenza","","","Hz","","","50"]
["","Tensione","","","V","","","220-240"]