{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9 / RXS50L2V1B"]
["Capacità di Raffrescamento","Min.","","kW","1.7"]
["","Max.","","kW","5.3"]
["","Nom.","","kW","5.0"]
["Attacchi tubazioni","Liquido","DE","mm","6.35"]
["","Gas","DE","mm","12.7"]
["","Scarico","OD","mm","VP20 (Diametro esterno 26, Diametro interno 20)"]
["Efficienza nominale","Consumo energetico annuale","","kWh","825"]
["","EER","","","3.03"]
["","COP","","","3.10"]
["","Classe energetica","Raffreddamento","","B"]
["","","Riscaldamento","","D"]
["Capacità di riscaldamento","Nom.","","kW","5.8"]
["","Min.","","kW","1.7"]
["","Max.","","kW","6.0"]
["Note","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["","","","","(2) - 230V"]
["","","","","(3) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale"]