{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","36","37","37","38"]
["","","Nom.","dBA","34","35","35","36"]
["","","Medio","dBA","31","32","33","34"]
["","Raffrescamento","Medio","dBA","34","35","35","36"]
["","","Bassa","dBA","31","32","33","34"]
["","","Alta","dBA","36","37","37","38"]
["Accessori standard","Tubo isolamento termico","","","2","2","2","2"]
["","Materiale di fissaggio cavi","","","7","7","7","7"]
["","Fascetta tubo flessibile","","","1","1","1","1"]
["","Tubo flessibile di scarico","","","1","1","1","1"]
["","Rondella","","","8","8","8","8"]
["","Materiale di tenuta (grande)","","","1","1","1","1"]
["","Materiale di tenuta (piccolo)","","","1","1","1","1"]
["","Boccola in resina","","","1","1","1","1"]
["","Viti","","","2","2","2","2"]
["","Barra di cablaggio","","","2","2","2","2"]
["Sistemi di controllo","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Piping connections","Liquido","DE","mm","6.35","6.35","6.35","9.52"]
["","Gas","DE","mm","9.50","12.7","12.7","15.9"]
["","Scarico","","","VP20","VP20","VP20","VP20"]
["Livello potenza sonora","Raffrescamento","","dBA","53","54","54","55"]
["Dimensioni","Unità","Larghezza","mm","960","960","1,270","1,270"]
["","","Profondità","mm","690","690","690","690"]
["","","Altezza","mm","235","235","235","235"]
["Rivestimento","Materiale","","","Resina, lamiera","Resina, lamiera","Resina, lamiera","Resina, lamiera"]
["","Colour","","","Bianco","Bianco","Bianco","Bianco"]
["Peso","Unità","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frequenza","","Hz","50","50","50","50"]
["","Tensione","","V","220-240","220-240","220-240","220-240"]
["Note","","","","(1) - Consultare i disegni separati per i dati elettrici","(1) - Consultare i disegni separati per i dati elettrici","(1) - Consultare i disegni separati per i dati elettrici","(1) - Consultare i disegni separati per i dati elettrici"]