{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":16,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Capacità di Raffrescamento","Nom.","","kW","","","","","6.8","","","","","","","13.4"]
["Raffrescamento ambienti","SEER","","","6.95","5.10","5.10","5.10","6.86","5.10","5.10","5.10","6.11","5.10","6.01"]
["","Consumi energetici annuali","","kWh/a","343","467","467","467","347","652","652","652","545","824","699"]
["","Capacità","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","12.00","12.00"]
["","Classe di efficienza energetica","","","A++","B","B","B","A++","B","B","B","A++","B","A+"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","7.60","6.00","6.00","6.00","7.60","11.30","11.30","11.30","11.30","12.71","14.13"]
["","SCOP/A","","","4.32","3.80","3.80","3.80","4.32","3.80","3.80","3.80","4.61","3.80","4.23"]
["","Classe di efficienza energetica","","","A+","A","A","A","A+","A","A","A","A++","A","A+"]
["","Consumi energetici annuali","","kWh/a","2,463","2,211","2,211","2,211","2,463","4,164","4,164","4,164","3,432","4,683","4,677"]
["Efficienza nominale","Consumo energetico annuale","","kWh","","","","","890","","","","","","","2,025"]
["","EER","","","","","","","3.82","","","","","","","3.31"]
["","COP","","","","","","","4.13","","","","","","","3.63"]
["","Classe energetica","Raffreddamento","","","","","","A","","","","","","","A"]
["","","Riscaldamento","","","","","","A","","","","","","","A"]
["Capacità di riscaldamento","Nom.","","kW","","","","","7.5","","","","","","","15.5"]
["Note","","","","","","","","(1) - Il consumo energetico annuale è conforme alla direttiva 2002/31/CE sulla classificazione energetica","","","","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["","","","","","","","","(2) - I valori SEER e SCOP sono conformi alla norma europea EN 14825","","","","","","","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale"]