{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":12,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ50CBVEB / FHQ50CBVEB / RZQSG100L8Y1B","FHQ100CBVEB / RZQSG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQSG100L8Y1B","FHQ125CBVEB / RZQSG125L8Y1B","FHQ60CBVEB / FHQ60CBVEB / RZQSG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQSG125L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQSG125L8Y1B","FHQ140CBVEB / RZQSG140L7Y1B"]
["Capacità di Raffrescamento","Nom.","","kW","","9.5","","12.0","","","","13.4"]
["Raffrescamento ambienti","SEER","","","5.10","5.61","5.10","5.61","4.80","4.80","4.80"]
["","Consumi energetici annuali","","kWh/a","652","593","652","749","875","875","875"]
["","Capacità","Pdesign","kW","9.50","9.5","9.50","12","12.00","12.00","12.00"]
["","Classe di efficienza energetica","","","B","A+","B","A+","B","B","B"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","7.60","7.6","7.60","7.6","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.91","3.80","4.01","3.80","3.80","3.80"]
["","Classe di efficienza energetica","","","A","A","A","A+","A","A","A"]
["","Consumi energetici annuali","","kWh/a","2,800","2,722","2,800","2,654","2,800","2,800","2,800"]
["Efficienza nominale","Consumo energetico annuale","","kWh","","1,480","","2,075","","","","2,225"]
["","EER","","","","3.21","","2.89","","","","3.01"]
["","COP","","","","3.61","","3.62","","","","3.41"]
["","Classe energetica","Raffreddamento","","","A","","C","","","","B"]
["","","Riscaldamento","","","A","","A","","","","B"]
["Capacità di riscaldamento","Nom.","","kW","","10.8","","13.5","","","","15.5"]
["Note","","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","","","","(1) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["","","","","","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale","","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale","","","","(2) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale"]