{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":12,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N"]
[]
[]
[]
[]
["","","","","","FTXM20N2V1B","FTXM25N2V1B","FTXM35N2V1B","FTXM42N2V1B","FTXM50N2V1B","FTXM60N2V1B","FTXM71N2V1B"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.03","0.03","0.034","0.035","0.03","0.032","0.054"]
["","Riscaldamento","","Nom.","kW","0.025","0.026","0.026","0.036","0.032","0.035","0.06"]
["Rivestimento","Colore","","","","Bianco","Bianco","Bianco","Bianco","Bianco","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","294","294","294","294","300","300","300"]
["","","","Larghezza","mm","811","811","811","811","1040","1040","1040"]
["","","","Profondità","mm","272","272","272","272","295","295","295"]
["Peso","Unità","","","kg","10","10","10","10","14.5","14.5","14.5"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","11.1","11.1","12.3","12.6","16.1","17.1","17.6"]
["","","","Medio","m³/min","7.9","8.1","8.3","9.5","14.2","14.6","15"]
["","","","Bassa","m³/min","6","6.2","6.4","7.1","11.6","12","12.5"]
["","","","Funzionamento silenzioso","m³/min","4.4","4.4","4.6","4.6","8.1","9.1","10.1"]
["","","Riscaldamento","Alta","m³/min","10.8","10.8","10.8","13","17.1","17.7","18.4"]
["","","","Medio","m³/min","8.7","8.7","9","10.4","14.6","15.6","16.2"]
["","","","Bassa","m³/min","6.5","6.8","7.1","7.1","12.2","12.6","13"]
["","","","Funzionamento silenzioso","m³/min","5.3","5.3","5.3","5.3","10.7","11.2","11.9"]
["Potenza sonora","Raffrescamento","","","dBA","57","57","58","60","58","60","60"]
["","Riscaldamento","","","dBA","54","54","54","60","58","59","61"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","41","41","45","45","44","46","47"]
["Pressione sonora","Raffrescamento","","Medio","dBA","33","33","33","39","40","42","43"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25","25","29","30","36","37","38"]
["","","","Funzionamento silenzioso","dBA","19","19","19","21","27","30","32"]
["","Riscaldamento","","Alta","dBA","39","39","39","45","43","45","46"]
["Pressione sonora","Riscaldamento","","Medio","dBA","34","34","35","39","39","41","42"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","26","27","28","29","34","36","37"]
["","","","Funzionamento silenzioso","dBA","20","20","20","21","31","33","34"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","DE","mm","9.5","9.5","9.5","12.7","12.7","12.7","15.9"]
["","Scarico","","","","18","18","18","18","18","18","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Sistemi di controllo","Telecomando con cavo","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Accessori standard","Installation manual","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1"]
["Alimentazione","Nome","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50","50","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Sistemi di controllo","Telecomando infrarossi","","","","","","","","","ARC466A33","ARC466A33"]