{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB","FUA100AVEB9","FUA100AVEB","FUA125AVEB9","FUA125AVEB"]
["Capacità di Raffrescamento","Capacità totale","","Nom.","kW","","","","12.10","12.1"]
["Capacità di riscaldamento","Capacità totale","","Nom.","kW","","","","13.5","13.5"]
["Rivestimento","Colore","","","","Bianco frizzante","Bianco frizzante","Bianco frizzante","Bianco frizzante","Bianco frizzante"]
["","Materiale","","","","Resina","Resina","Resina","Resina","Resina"]
["Dimensioni","Unità","","Altezza","mm","198","198","198","198","198"]
["","","","Larghezza","mm","950","950","950","950","950"]
["","","","Profondità","mm","950","950","950","950","950"]
["Peso","Unità","","","kg","25.0","26.0","26.0","26.0","26"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","23.0","31.0","31.0","32.5","32.5"]
["","","","Medio","m³/min","19.5","25.5","25.5","26.5","26.5"]
["","","","Bassa","m³/min","16.0","20.0","20.0","20.5","20.5"]
["","","Riscaldamento","Alta","m³/min","23.0","31.0","31.0","32.5","32.5"]
["","","","Medio","m³/min","19.5","25.5","25.5","26.5","26.5"]
["","","","Bassa","m³/min","16.0","20.0","20.0","20.5","20.5"]
["Potenza sonora","Raffrescamento","","","dBA","59","64","64","65","65"]
["","Riscaldamento","","","dBA","59","","64"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","41","46","46","47","47"]
["Pressione sonora","Raffrescamento","","Medio","dBA","38","42","42","43","43"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","35","39","39","40","40"]
["","Riscaldamento","","Alta","dBA","41","46","46","47","47"]
["Pressione sonora","Riscaldamento","","Medio","dBA","38","42","42","43","43"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","35","39","39","40","40"]
["Attacchi tubazioni","Liquido","","DE","mm","9.52","9.52","9.52","9.52","9.52"]
["","Gas","","DE","mm","15.9","15.9","15.9","15.9","15.9"]
["","Scarico","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Prevalenza di scarico condensa","mm","","","","600","600","600","600","600"]
["Sistemi di controllo","Telecomando con cavo","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accessori standard","Installation manual","","","","1","1","1","1","1"]
["","Thermal insulation tube","","","","3","3","3","3","3"]
["","Non woven fabric","","","","1","1","1","1","1"]
["","Drain joint","","","","1","1","1","1","1"]
["","Hose band","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5","5","5"]
["","Sealing material","","","","4","4","4","4","4"]
["","Tie-wraps","","","","10","10","10","10","10"]
["","Washer","","","","8","8","8","8","8"]
["","Washer fixing plate","","","","1","1","1","1","1"]