{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":8,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.02","0.02","0.03"]
["","Riscaldamento","","Nom.","kW","0.02","0.03","0.03"]
["Rivestimento","Colore","","","","Bianco","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","600","600","600"]
["","","","Larghezza","mm","750","750","750"]
["","","","Profondità","mm","238","238","238"]
["Peso","Unità","","","kg","17","17","17"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³;/min","8.7","9.2","11.6"]
["","","","Medio","m³;/min","7","7","9"]
["","","","Bassa","m³;/min","4.9","4.9","6.6"]
["","","","Funzionamento silenzioso","m³;/min","4.1","4.1","5.4"]
["","","Riscaldamento","Alta","m³;/min","9.2","9.8","12.8"]
["","","","Medio","m³;/min","7.2","7.2","10"]
["","","","Bassa","m³;/min","5.6","5.6","8.4"]
["","","","Funzionamento silenzioso","m³;/min","4.1","4.1","5.9"]
["Potenza sonora","Raffrescamento","","","dBA","52","53","61"]
["","Riscaldamento","","","dBA","52","53","62"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","38","39","44"]
["Pressione sonora","Raffrescamento","","Medio","dBA","32","32","38"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25","25","31"]
["","","","Funzionamento silenzioso","dBA","20","20","27"]
["","Riscaldamento","","Alta","dBA","38","39","46"]
["Pressione sonora","Riscaldamento","","Medio","dBA","32","32","40"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","25","25","35"]
["","","","Funzionamento silenzioso","dBA","19","19","29"]
["Refrigerante","GWP","","","","675","675","675"]
["Attacchi tubazioni","Liquido","","DE","mm","6.4","6.4","6.4"]
["","Gas","","DE","mm","9.5","9.5","12.7"]
["","Scarico","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sistemi di controllo","Telecomando infrarossi","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Telecomando con cavo","","","","BRC073A1","BRC073A1","BRC073A1"]
["Accessori standard","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Alimentazione","Nome","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240"]
["Note","","","","","(1) - Raffreddamento: temp. interna 27°CBS, 19°CBU, temp. esterna 35°CBS, 24°CBU; lunghezza equivalente delle tubazioni: 5m","(1) - Raffreddamento: temp. interna 27°CBS, 19°CBU, temp. esterna 35°CBS, 24°CBU; lunghezza equivalente delle tubazioni: 5m","(1) - Raffreddamento: temp. interna 27°CBS, 19°CBU, temp. esterna 35°CBS, 24°CBU; lunghezza equivalente delle tubazioni: 5m"]
["","","","","","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 5m","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 5m","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 5m"]
["Accessori standard","FVXM50B2V1B","","","","","","1"]