{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":11,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXV-ATV3R"]
[]
[]
[]
[]
["","","","","","FWXV10ABTV3R","FWXV15ABTV3R","FWXV20ABTV3R","FWXV10AATV3R (Archived)","FWXV15AATV3R (Archived)","FWXV20AATV3R (Archived)"]
["Dimensioni","Unità","","Larghezza","mm","","","","999","1,200","1,400"]
["","","","Profondità","mm","","","","135","135","135"]
["","","","Altezza","mm","","","","601","601","601"]
["Rivestimento","Colore","","","","","","","RAL 9003","RAL 9003","RAL 9003"]
["Peso","Unità","","","kg","","","","20.0","23.0","26.0"]
["Power supply","Fase","","","","","","","1~","1~","1~"]
["","Frequenza","","","Hz","","","","50","50","50"]
["","Tensione","","","V","","","","230","230","230"]
["Capacità di raffrescamento","7/12°C","","Min.","kW","0.78","1.10","1.13"]
["","","","Med.","kW","1.11","1.65","1.98"]
["","","","Capacità di raffrescamento-=-7/12°C-=-Max.-=-kW","kW","1.62","2.64","2.99"]
["Capacità di raffrescamento sensibile","7/12°C","","Min.","kW","0.58","0.82","0.85"]
["","","","Med.","kW","0.71","1.15","1.55"]
["","","","Max.","kW","1.25","1.91","2.33"]
["Capacità di riscaldamento","45/40°C","","Min.","kW","0.87","1.12","1.11"]
["","","","Med.","kW","1.27","1.83","2.32"]
["","","","Max.","kW","1.96","2.86","3.50"]
["Potenza assorbita","Min.","","","kW","0.01","0.01","0.01"]
["","Med.","","","kW","0.01","0.01","0.01"]
["","Max.","","","kW","0.02","0.03","0.03"]
["Velocità del ventilatore","Min.","","","giri/min","720.00","720.00","720.00"]
["","Med.","","","giri/min","1220.00","1220.00","1220.00"]
["","Max.","","","giri/min","1700.00","1700.00","1700.00"]
["Rivestimento","Colore","","","","RAL 9003","RAL 9003","RAL 9003"]
["","Materiale","","","","Lamiera","Lamiera","Lamiera"]
["Dimensioni","Unità","","Altezza","mm","601","601","601"]
["","","","Larghezza","mm","999","1199","1399"]
["","","","Profondità","mm","135","135","135"]
["","Unità imballata","","Altezza","mm","690","690","690"]
["","","","Larghezza","mm","1230","1430","1630"]
["","","","Profondità","mm","210","210","210"]
["Peso","Unità","","","kg","20","23","26"]
["","Unità imballata","","","kg","21","24","27"]
["Imballaggio","Materiale","","","","Cartone","Cartone","Cartone"]
["Guarnizione","Peso","","","kg","1","1","1"]
["Scambiatore di calore","Quantità","","","","1","1","1"]
["","Volume batteria interna","","","l","0.8","1.1","1.5"]
["","Carica","","Pressione d'esercizio","bar","10","10","10"]
["Circuito idraulico","Diametro attacchi delle tubazioni","","","in","3/4","3/4","3/4"]
["","Materiale tubazione","","","","RAME","RAME","RAME"]
["","Pressione","Riscaldamento","Max.","bar","10","10","10"]
["Circuito idraulico - perdita di carico dell’acqua","Riscaldamento","45/40°C","Min.","kPa","7.00","9.00","8.00"]
["","","","Med.","kPa","8.00","14.00","15.00"]
["","","","Max.","kPa","11.00","23.00","22.00"]
["","Raffrescamento","7/12°C","Min.","kPa","7.00","9.00","8.00"]
["","","","Med.","kPa","8.00","14.00","15.00"]
["","","","Max.","kPa","11.00","23.00","22.00"]
["Circuito idraulico - portata d’acqua","Riscaldamento","45/40°C","Min.","kg/h","150.00","200.00","190.00"]
["","","","Med.","kg/h","220.00","320.00","400.00"]
["","","","Max.","kg/h","340.00","500.00","610.00"]
["","Raffrescamento","7/12°C","Min.","kg/h","130.00","190.00","190.00"]
["","","","Med.","kg/h","190.00","280.00","340.00"]
["","","","Max.","kg/h","280.00","450.00","510.00"]
["Potenza sonora","Min.","","","dBA","40","42","43"]
["","Med.","","","dBA","47","49","50"]
["Livello di potenza sonora","Max.","","","dBA","56.0","57.0","58.0"]
["Campo di funzionamento","Riscaldamento","Lato acqua","Min.","°C","30","30","30"]
["","","","Max.","°C","85","85","85"]
["","Raffrescamento","Lato acqua","Min.","°C","5","5","5"]
["","","","Max.","°C","18","18","18"]
["","Installazione in spazi interni","T. esterna","Min.","°CBS","0","0","0"]
["","","","Max.","°CBS","45","45","45"]
["Sistemi di controllo","Telecomando infrarossi","","","","No","No","No"]
["","Integrato sull'unità interna","","","","Sì","Sì","Sì"]
["Alimentazione","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","230","230","230"]
["Potenza assorbita","Max.","","","W","19","25","31"]
["","Stand-by","","","W","3","4","5"]
["Corrente","Max. corrente di funzionamento","","Riscaldamento","A","0.15","0.21","0.27"]
["","","","Raffresc.","A","0.15","0.21","0.27"]