{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-A"]
[]
[]
[]
[]
["","","","","","FXMQ200AXVMB","FXMQ250AXVMB"]
["Capacità di raffrescamento","Capacità totale","","Ad alta velocità del ventilatore","kW","22.4","28.0"]
["Capacità di riscaldamento","Capacità totale","","Ad alta velocità del ventilatore","kW","25.0","31.5"]
["Potenza assorbita - 50Hz","Raffrescamento","","Ad alta velocità del ventilatore","kW","0.54","0.65"]
["","Riscaldamento","","Ad alta velocità del ventilatore","kW","0.54","0.65"]
["Dimensioni","Unità","","Altezza","mm","470","470"]
["","","","Larghezza","mm","1490","1490"]
["","","","Profondità","mm","1100","1100"]
["Peso","Unità","","","kg","105","115"]
["Rivestimento","Colore","","","","Non verniciato","Non verniciato"]
["","Materiale","","","","Lamiera in acciaio zincato","Lamiera in acciaio zincato"]
["Ventilatore","Portata d'aria - 50 Hz","Raffrescamento","Ad alta velocità del ventilatore","m³/min","62","74"]
["","","","A velocità del ventilatore bassa","m³/min","41","52"]
["","Prevalenza - 50Hz","","Alta","Pa","250","250"]
["","","","Bassa","Pa","50","50"]
["","Prevalenza - 60Hz","","Alta","Pa","250","250"]
["","","","Bassa","Pa","50","50"]
["Refrigerante","Tipo","","","","R-410A","R-410A"]
["","GWP","","","","2087.5","2087.5"]
["Livello di potenza sonora","Raffrescamento","","Ad alta velocità del ventilatore","dBA","75.0","76.0"]
["Pressione sonora","Raffrescamento","","Ad alta velocità del ventilatore","dBA","48.0","48.0"]
["","","","A velocità del ventilatore media","dBA","46.5","46.5"]
["","","","Pressione sonora-=-Raffrescamento-=-A velocità del ventilatore bassa-=-dBA","dBA","45.0","45.0"]
["","Riscaldamento","","Ad alta velocità del ventilatore","dBA","48.0","48.0"]
["","","","A velocità del ventilatore media","dBA","46.5","46.5"]
["","","","A velocità del ventilatore bassa","dBA","45.0","45.0"]
["Attacchi tubazioni","Liquido","","Tipo","","Attacco a cartella","Attacco a cartella"]
["","","","DE","mm","9.5","9.5"]
["","Gas","","Tipo","","Flangia","Flangia"]
["","","","DE","mm","19.1","22.2"]
["","Scarico","","","","BSP1","BSP1"]
["Accessori standard","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","1","1"]
["","Spring washer","","","","2","2"]
["","Hexagon head screw","","","","2","2"]
["","Plain washer","","","","8","8"]
["","Hexagon head screw with washer","","","","49","49"]
["","Gas connection pipe","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["Alimentazione","Nome","","","","VM","VM"]
["","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50/60","50/60"]
["","Tensione","","","V","220-240/220-230","220-240/220-230"]
["Corrente - 50Hz","Portata massima del fusibile (MFA)","","","A","6","6"]