{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimensioni","Unità","","Altezza","mm","870","870"]
["","","","Larghezza","mm","1,100","1,100"]
["","","","Profondità","mm","460","460"]
["Peso","Unità","","","kg","117","117"]
["Compressore","Tipo","","","","Compressore ermetico Scroll","Compressore ermetico Scroll"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-20","-20"]
["","","","Max.","°CBS","46","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-20","-20"]
["","","","Max.","°CBU","15","15"]
["Sound power level","Raffrescamento","","","dBA","73","76"]
["","Riscaldamento","","","dBA","76 (1)","79 (1)"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","53","57"]
["","Riscaldamento","","Nom.","dBA","60","63"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carica","","","kg","5","5"]
["","GWP","","","","675","675"]
["Collegamenti tubazioni","Liquido","","DE","mm","9.52","9.52"]
["","Gas","","DE","mm","22.2","22.2"]
["","Lunghezza tubazioni","Max.","est. - int.","m","100","100"]
["","","Sistema","Senza carica","m","30","30"]
["","Carica di refrigerante aggiuntivo","","","kg/m","Consultare il manuale di installazione","Consultare il manuale di installazione"]
["Accessori standard","Manuale di installazione","","","","1","1"]
["","Misure di sicurezza generali","","","","1","1"]
["","Fascette","","","","2","2"]
["","Rimuovere l’etichetta F-gas","","","","1","1"]
["","Raccordi","","","","6","6"]
["Power supply","Fase","","","","3~","3~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","380-415","380-415"]
["Corrente - 50Hz","Portata massima del fusibile (MFA)","","","A","20","20"]
["Note","","","","","(1) - Conforme a ENER Lot 21","(1) - Conforme a ENER Lot 21"]