{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Dimensioni","Unità","","Altezza","mm","734","734","734"]
["","","","Larghezza","mm","870","870","870"]
["","","","Profondità","mm","373","373","373"]
["Peso","Unità","","","kg","52","52","52"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-20","-20","-20"]
["","","","Max.","°CBS","52","52","52"]
["","Riscaldamento","T. esterna","Min.","°CBU","-21","-21","-21"]
["","","","Max.","°CBU","18","18","18"]
["Potenza sonora","Raffrescamento","","","dBA","62","63","64"]
["","Riscaldamento","","","dBA","62","63","64"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","48","49","50"]
["","Riscaldamento","","Nom.","dBA","48","49","50"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32"]
["","Carica","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","1.05","1.05","1.05"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35","6.35"]
["","Gas","","DE","mm","9.52","12.7","12.7"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","50","50","50"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 30m)","0,02 (per lunghezza delle tubazioni superiore ai 30m)","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Dislivello","int. - est.","Max.","m","30","30","30"]
["Accessori standard","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Alimentazione","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240"]
["Note","","","","","(1) - Per informazioni sul campo di funzionamento consultare i disegni separati","(1) - Per informazioni sul campo di funzionamento consultare i disegni separati","(1) - Per informazioni sul campo di funzionamento consultare i disegni separati"]
["","","","","","(2) - Consultare i disegni separati per i dati elettrici","(2) - Consultare i disegni separati per i dati elettrici","(2) - Consultare i disegni separati per i dati elettrici"]
["","","","","","(3) - Contiene gas fluorurati a effetto serra","(3) - Contiene gas fluorurati a effetto serra","(3) - Contiene gas fluorurati a effetto serra"]
["Accessori standard","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]