{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimensioni","Unità","","Altezza","mm","1,680"]
["","","","Larghezza","mm","930"]
["","","","Profondità","mm","765"]
["Peso","Unità","","","kg","183.0"]
["Compressore","Tipo","","","","Compressore ermetico Scroll"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-5.0"]
["","","","Max.","°CBS","46.0"]
["","Riscaldamento","T. esterna","Min.","°CBU","-15.0"]
["","","","Max.","°CBU","15.0"]
["Sound power level","Raffrescamento","","","dBA","78.0"]
["","Riscaldamento","","","dBA","78.0"]
["Refrigerante","Tipo","","","","R-410A"]
["","Carica","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Collegamenti tubazioni","Liquido","","DE","mm","9.52"]
["","Gas","","DE","mm","22.2"]
["","Lunghezza tubazioni","Max.","est. - int.","m","100"]
["","","Sistema","Senza carica","m","30"]
["Accessori standard","Manuale di installazione","","","","1"]
["","Raccordi","","","","4"]
["Power supply","Fase","","","","3N~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","380-415"]
["Corrente - 50Hz","Portata massima del fusibile (MFA)","","","A","25"]
["Note","","","","","(1) - L'alimentazione all'unità interna FDQ è separata"]
["","","","","","(2) - Vedi i disegni separati per i dati elettrici"]
["Dimensioni","Unità","","Altezza","mm","","1680"]
["","","","Larghezza","mm","","930"]
["","","","Profondità","mm","","765"]
["Peso","Unità","","","kg","","184.0"]
["Compressore","Tipo","","","","","Compressore ermetico tipo Scroll"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","","-5.0"]
["","","","Max.","°CBS","","46.0"]
["","Riscaldamento","T. esterna","Min.","°CBU","","-15.0"]
["","","","Max.","°CBU","","15.0"]
["Potenza sonora","Raffrescamento","","","dBA","","78.0"]
["","Riscaldamento","","","dBA","","78.0"]
["Refrigerante","Carica","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","","19.4"]
["Attacchi tubazioni","Liquido","","DE","mm","","12.70"]
["","Gas","","DE","mm","","22.2"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","100"]
["","","Sistema","Senza carica","m","","30"]
["Accessori standard","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Alimentazione","Frequenza","","","Hz","","50"]
["Corrente - 50Hz","Portata massima del fusibile (MFA)","","","A","","25"]