{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H519W"]
[]
[]
[]
[]
["","","","","BRC1H519W."]
["Guarnizione","Materiale","","","Cartone"]
["","Peso","","kg","0.0850"]
["Temperatura esterna","Umidità relativa <","","%","95"]
["Dimensioni","Unità imballata","Larghezza","mm","217"]
["","","Altezza","mm","50"]
["","","Profondità","mm","161"]
["","Unità","Larghezza","mm","85"]
["","","Profondità","mm","25"]
["","","Altezza","mm","85"]
["Rivestimento","Coperchio pulsantiera","","","No"]
["","Colore","","","Bianco"]
["","LED di funzionamento","Colore","","Blue status indicator"]
["LCD","Tipo","","","100 x 150 dots"]
["","Retroilluminazione","Colore","","Bianco"]
["","Dimensioni","Larghezza","mm","28.0"]
["","","Altezza","mm","40.7"]
["Peso","Unità imballata","","kg","0.317"]
["","Unità","","kg","0.110"]
["Collegamenti elettrici","Lunghezza cablaggio","Max.","m","500"]